Overview | Top | Package | Element
| Interface UML Documentation

Summary:Attributes Properties | Detail:Attributes

Interface
Class Outbound Message Recipient

Attributes
| Sequence Number | Independent counter for message sequence, which is available once per party technical address
<<Entity>> <Class> Party Technical Address | was sent to |
<<Boundary>> <Class> Outbound File Delivery | outbound File Delivery |
<<Boundary>> <Class> Outbound Message Delivery | outbound Message Delivery |

Properties:

Is Abstract | false
Is Active | false
Is Leaf | false
Name | Outbound Message Recipient
Namespace | <Package> Interface
Owner | <Package> Interface
Package | <Package> Interface
Qualified Name | T2S Data Model::Interface::Outbound Message Recipient
Stereotype | Boundary
Visibility | Public

Attribute Details

outbound File Delivery

    Private <<Boundary>> <Class> Outbound File Delivery outbound File Delivery

Constraints:
Properties:

  Aggregation | None
  Association | <Association> A_outbound Message Recipient_outbound File Delivery
  Class | <<Boundary>> <Class> Outbound Message Recipient
  Is Composite | false
  Is Derived | false
  Is Derived Union | false
  Is Leaf | false
  Is Ordered | false
  Is Read Only | false
  Is Static | false
  Is Unique | true
  Lower | 0
  Lower Value | <Literal Integer> 0
  Multiplicity | *
  Name | outbound File Delivery
  Namespace | <<Boundary>> <Class> Outbound Message Recipient
  Opposite | <Property> outbound Message Recipient : Outbound Message Recipient [0..1]
  Owner | <<Boundary>> <Class> Outbound Message Recipient
  Qualified Name | T2S Data Model::Interface::Outbound Message Recipient::outbound File Delivery
  Type | <<Boundary>> <Class> Outbound File Delivery
  Upper | *
  Upper Value | <Literal Unlimited Natural> *
  Visibility | Private

outbound Message Delivery

    Private <<Boundary>> <Class> Outbound Message Delivery outbound Message Delivery

Constraints:
Properties:

  Aggregation | None
  Association | <Association> A_outbound Message Recipient_outbound Message Delivery
  Class | <<Boundary>> <Class> Outbound Message Recipient
  Is Composite | false
  Is Derived | false
  Is Derived Union | false
  Is Leaf | false
  Is Ordered | false
  Is Read Only | false
  Is Static | false
  Is Unique | true
  Lower | 0
  Lower Value | <Literal Integer> 0
  Multiplicity | *
  Name | outbound Message Delivery
  Namespace | <<Boundary>> <Class> Outbound Message Recipient
  Opposite | <Property> outbound Message Recipient : Outbound Message Recipient [0..1]
  Owner | <<Boundary>> <Class> Outbound Message Recipient
  Qualified Name | T2S Data Model::Interface::Outbound Message Recipient::outbound Message Delivery
  Type | <<Boundary>> <Class> Outbound Message Delivery
  Upper | *
  Upper Value | <Literal Unlimited Natural> *
  Visibility | Private

Sequence Number

    Public Sequence Number

  Independent counter for message sequence, which is available once per party technical address

Constraints:
Properties:

  Aggregation | None
  Class | <<Boundary>> <Class> Outbound Message Recipient
  Is Composite | false
  Is Derived | false
  Is Derived Union | false
  Is Leaf | false
  Is Ordered | false
  Is Read Only | false
  Is Static | false
  Is Unique | true
  Lower | 1
  Multiplicity | 1
  Name | Sequence Number
  Namespace | <<Boundary>> <Class> Outbound Message Recipient
  Owner | <<Boundary>> <Class> Outbound Message Recipient
  Qualified Name | T2S Data Model::Interface::Outbound Message Recipient::Sequence Number
  Upper | 1
  Visibility | Public

was sent to

    Private <<Entity>> <Class> Party Technical Address was sent to

Constraints:
Properties:

  Aggregation | None
  Association | <Association> A_received_was sent to
  Class | <<Boundary>> <Class> Outbound Message Recipient
  Is Composite | false
  Is Derived | false
  Is Derived Union | false
  Is Leaf | false
  Is Ordered | false
  Is Read Only | false
  Is Static | false
  Is Unique | true
  Lower | 1
  Lower Value | <Literal Integer> 1
  Multiplicity | 1
  Name | was sent to
  Namespace | <<Boundary>> <Class> Outbound Message Recipient
  Opposite | <Property> received : Outbound Message Recipient [0..*]
  Owner | <<Boundary>> <Class> Outbound Message Recipient
  Qualified Name | T2S Data Model::Interface::Outbound Message Recipient::was sent to
  Type | <<Entity>> <Class> Party Technical Address
  Upper | 1
  Upper Value | <Literal Unlimited Natural> 1
  Visibility | Private

Overview | Top | Package | Element
| Interface UML Documentation

Summary:Attributes Properties | Detail:Attributes