Overview | Top | Package | Element
| Party Data Management UML Documentation

Summary:Attributes Properties | Detail:Attributes

Static Data Management::Party Data Management
Class Party Technical Address

This entity includes information related to all technical addresses defined for a Party {T2S.16.700}. Each Party Technical Address uniquely identifies a possible recipient technical address the Party can use in the message subscription service.Each Party Technical Address is linked to its relevant Party and to one or many Network Services.

Attributes
<Primitive Type> String | Technical Address | Unique technical address of a party in T2S (e.g. a BIC, a distinguished name, an IP address).
<<Boundary>> <Class> Inbound Communication | delivered |
<<Boundary>> <Class> Outbound Message Recipient | received |
<<Entity>> <Class> Routing | defines destination for message flow according to |
<<Entity>> <Class> Network Service | is defined for |

Properties:

Is Abstract | false
Is Active | false
Is Leaf | false
Name | Party Technical Address
Namespace | <Package> Party Data Management
Owner | <Package> Party Data Management
Package | <Package> Party Data Management
Qualified Name | T2S Data Model::Static Data Management::Party Data Management::Party Technical Address
Stereotype | Entity
Visibility | Public

Attribute Details

defines destination for message flow according to

    Private <<Entity>> <Class> Routing defines destination for message flow according to

Constraints:
Properties:

  Aggregation | None
  Association | <Association> A_defines destination for message flow according to_directs message flow to
  Class | <<Entity>> <Class> Party Technical Address
  Is Composite | false
  Is Derived | false
  Is Derived Union | false
  Is Leaf | false
  Is Ordered | false
  Is Read Only | false
  Is Static | false
  Is Unique | true
  Lower | 0
  Lower Value | <Literal Integer> 0
  Multiplicity | *
  Name | defines destination for message flow according to
  Namespace | <<Entity>> <Class> Party Technical Address
  Opposite | <Property> directs message flow to : Party Technical Address
  Owner | <<Entity>> <Class> Party Technical Address
  Qualified Name | T2S Data Model::Static Data Management::Party Data Management::Party Technical Address::defines destination for message flow according to
  Type | <<Entity>> <Class> Routing
  Upper | *
  Upper Value | <Literal Unlimited Natural> *
  Visibility | Private

delivered

    Private <<Boundary>> <Class> Inbound Communication delivered

Constraints:
Properties:

  Aggregation | None
  Association | <Association> A_was sent by_delivered
  Class | <<Entity>> <Class> Party Technical Address
  Is Composite | false
  Is Derived | false
  Is Derived Union | false
  Is Leaf | false
  Is Ordered | false
  Is Read Only | false
  Is Static | false
  Is Unique | true
  Lower | 0
  Lower Value | <Literal Integer> 0
  Multiplicity | *
  Name | delivered
  Namespace | <<Entity>> <Class> Party Technical Address
  Opposite | <Property> was sent by : Party Technical Address
  Owner | <<Entity>> <Class> Party Technical Address
  Qualified Name | T2S Data Model::Static Data Management::Party Data Management::Party Technical Address::delivered
  Type | <<Boundary>> <Class> Inbound Communication
  Upper | *
  Upper Value | <Literal Unlimited Natural> *
  Visibility | Private

is defined for

    Private <<Entity>> <Class> Network Service is defined for

Constraints:
Properties:

  Aggregation | None
  Association | <Association> A_is defined for_party Technical Address
  Class | <<Entity>> <Class> Party Technical Address
  Is Composite | false
  Is Derived | false
  Is Derived Union | false
  Is Leaf | false
  Is Ordered | false
  Is Read Only | false
  Is Static | false
  Is Unique | true
  Lower | 1
  Lower Value | <Literal Integer> 1
  Multiplicity | 1..*
  Name | is defined for
  Namespace | <<Entity>> <Class> Party Technical Address
  Owner | <<Entity>> <Class> Party Technical Address
  Qualified Name | T2S Data Model::Static Data Management::Party Data Management::Party Technical Address::is defined for
  Type | <<Entity>> <Class> Network Service
  Upper | *
  Upper Value | <Literal Unlimited Natural> *
  Visibility | Private

received

    Private <<Boundary>> <Class> Outbound Message Recipient received

Constraints:
Properties:

  Aggregation | None
  Association | <Association> A_received_was sent to
  Class | <<Entity>> <Class> Party Technical Address
  Is Composite | false
  Is Derived | false
  Is Derived Union | false
  Is Leaf | false
  Is Ordered | false
  Is Read Only | false
  Is Static | false
  Is Unique | true
  Lower | 0
  Lower Value | <Literal Integer> 0
  Multiplicity | *
  Name | received
  Namespace | <<Entity>> <Class> Party Technical Address
  Opposite | <Property> was sent to : Party Technical Address
  Owner | <<Entity>> <Class> Party Technical Address
  Qualified Name | T2S Data Model::Static Data Management::Party Data Management::Party Technical Address::received
  Type | <<Boundary>> <Class> Outbound Message Recipient
  Upper | *
  Upper Value | <Literal Unlimited Natural> *
  Visibility | Private

Technical Address

    Public <Primitive Type> String Technical Address

  Unique technical address of a party in T2S (e.g. a BIC, a distinguished name, an IP address).

Constraints:
Properties:

  Aggregation | None
  Class | <<Entity>> <Class> Party Technical Address
  Is Composite | false
  Is Derived | false
  Is Derived Union | false
  Is Leaf | false
  Is Ordered | false
  Is Read Only | false
  Is Static | false
  Is Unique | true
  Lower | 1
  Multiplicity | 1
  Name | Technical Address
  Namespace | <<Entity>> <Class> Party Technical Address
  Owner | <<Entity>> <Class> Party Technical Address
  Qualified Name | T2S Data Model::Static Data Management::Party Data Management::Party Technical Address::Technical Address
  Type | <Primitive Type> String
  Upper | 1
  Visibility | Public

Overview | Top | Package | Element
| Party Data Management UML Documentation

Summary:Attributes Properties | Detail:Attributes